Removing a digital signature is possible with firmware 31 july, you can upgrade your firmware to 31 july 2019 from bitmain web page: https://file12.bitmain.com/shop-product/firmware/8199e72b-929f-4a66-a498-3e1e76b0ba89/2019/08/08/22/Antminer-S9-xilinx-201907311618-autofreq-user-Update2UBI-NF-sig.tar.gz and after you can use our program to remove signature
 
You can remove signature with sd card also (you can download from our web page)

If you have problem with program try to put the program to the disc c:
and run files without administration rights

1. You need to use file signature.exe
2. Set scan range IP START and IP END. If you want scan from 192.168.1.2 to 192.168.1.40 - set IPSTART=192.168.1.1 IPEND=192.168.1.40	
3. Set up asic password
4. confirm the file with vnish firmware you want to flash
5. confirm the configuration file and press enter, the program will start to remove signature and flash the basic by vanish firmware.
6. Go to ASIC via IP (only numbers, for example 192.168.1.2) and press ctrl + f5 to reset the cache if you see the old firmware




Снятие цифровой подписи возможно только c прошивки 31 июля 2019 года, вы можете обновить версию прошивки до 31 июля 2019 скачав ее с сайта bitmain : https://file12.bitmain.com/shop-product/firmware/8199e72b-929f-4a66-a498-3e1e76b0ba89/2019/08/08/22/Antminer-S9-xilinx-201907311618-autofreq-user-Update2UBI-NF-sig.tar.gz и далее снять защиту

Также вы можете снять цифровую подпись используя наш образ для SD карты (скачать образ можете с нашего сайта)

Если при использовании программы вылетает ошибка то скопируйте папку с программой  на диск C: и запустите ее без прав Администратора

1.Запустите файл signature.exe
2.Установить диапазон сканирования IP START и IP END. Если вы хотите сканировать с 192.168.1.1 по 192.168.1.40 - установите IPSTART=192.168.1.1 IPEND=192.168.1.40.
3.Задайте пароль от асика
4.Подтвердите файл с прошивкой vnish 
5.Подтвердите конфигурацию и нажмите enter для старта
6.Зайдите в асик через IP (только цифры, например 192.168.1.2) и нажмите ctrl+f5 чтобы сбросить кэш если вы видите старую прошивку